TOC · Work · Menu · Tools

### Fill sectors

Write a hex pattern or a file pattern to a sector range of the device.

The maximum size of the hex pattern is 8 bytes. Use files for larger patterns.

Sector alignment. If the option is checked and the next pattern copy does not fit into the sector entirely then pattern writing starts from the beginning of the next sector. Otherwise patterns are being written consistently regardless of sector boundaries.